COR PATHWAY 360
Equipment Pre Use Inspection
Completed by the operator, before the equipment is put to work
The operator inspects the equipment because the operator is the person who will be on it when something fails. Sign it because you looked, not because the shift is starting.
A defect that affects safe operation means the equipment does not run until it is repaired. Tag it out and tell your supervisor. Nobody is expected to operate equipment with a safety defect.
Check this yourself. Always follow the manufacturer's inspection requirements for the specific machine, and any additional requirements your jurisdiction sets for that equipment class. This form is a general operator check, not a replacement for the operator manual.
Equipment and operator
	Equipment type
	

	Unit number
	

	Make and model
	

	Hour meter or odometer reading
	

	Operator name
	

	Date and time
	

	Site or location
	

	Operator is trained and authorized for this equipment
	


How to mark each item
OK: checked and satisfactory.
D: defect found. Record it in the defect table and decide whether the equipment can run.
N/A: not fitted to this machine.
1. Walk around, before starting
	#
	Item
	S
	D
	N
	Comment

	1
	No fluid leaks under or on the machine
	
	
	
	

	2
	Engine oil, coolant, hydraulic and fuel levels correct
	
	
	
	

	3
	Tires condition and pressure, or tracks and undercarriage condition
	
	
	
	

	4
	Wheel nuts and rims secure and undamaged
	
	
	
	

	5
	No visible cracks in the frame, boom, bucket or attachment
	
	
	
	

	6
	Attachment secure, pins and locks in place
	
	
	
	

	7
	Hoses and lines free of chafing, bulges and leaks
	
	
	
	

	8
	Steps, grab handles and walking surfaces present and clean
	
	
	
	

	9
	Guards, covers and shields in place and secure
	
	
	
	

	10
	Counterweight secure, if fitted
	
	
	
	

	11
	No debris or combustible build up around the engine or exhaust
	
	
	
	


2. Operator station
	#
	Item
	S
	D
	N
	Comment

	1
	Cab glass clean and undamaged, mirrors present and adjusted
	
	
	
	

	2
	Seat secure, seat belt present and functional
	
	
	
	

	3
	Rollover or falling object protective structure undamaged and unmodified
	
	
	
	

	4
	Controls move freely, return to neutral, and are correctly labelled
	
	
	
	

	5
	Gauges, warning lights and alarms functional
	
	
	
	

	6
	Horn functional
	
	
	
	

	7
	Backup alarm functional
	
	
	
	

	8
	Lights, beacon and work lights functional
	
	
	
	

	9
	Windshield wipers and washer functional
	
	
	
	

	10
	Heater and defroster functional
	
	
	
	

	11
	Cab clear of loose items that could interfere with the controls
	
	
	
	

	12
	Operator manual present in the cab
	
	
	
	


3. Safety and emergency equipment
	#
	Item
	S
	D
	N
	Comment

	1
	Fire extinguisher present, charged, secured and inspection tag current
	
	
	
	

	2
	First aid kit present and stocked
	
	
	
	

	3
	Emergency stop functional
	
	
	
	

	4
	Isolation or battery disconnect accessible and functional
	
	
	
	

	5
	Wheel chocks present, if required
	
	
	
	

	6
	Spill kit present, if required
	
	
	
	

	7
	Communication device working, and coverage confirmed for the work area
	
	
	
	

	8
	Fall protection anchor points present and undamaged, if required
	
	
	
	


4. After starting
	#
	Item
	S
	D
	N
	Comment

	1
	No unusual noise, smoke or vibration
	
	
	
	

	2
	Warning lights all cleared after start up
	
	
	
	

	3
	Service brake holds, tested before moving
	
	
	
	

	4
	Park brake holds on a grade
	
	
	
	

	5
	Steering responds normally in both directions
	
	
	
	

	6
	Hydraulic functions operate smoothly, no drift under load
	
	
	
	

	7
	Load hold and lowering controls function correctly
	
	
	
	

	8
	Outriggers or stabilizers deploy and hold, if fitted
	
	
	
	


Defects found
	Item
	Defect
	Affects safe operation, yes or no
	Tagged out
	Reported to
	Date reported

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Decision
	Equipment is safe to operate, yes or no
	

	If no, action taken
	

	Tag out number, if applied
	

	Supervisor notified, name and time
	


Repairs and return to service
	Defect
	Repair performed
	Repaired by
	Date
	Returned to service by

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Sign off
	Operator
	Supervisor

	
	


	Date
	Date
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