COR PATHWAY 360
Field Level Hazard Assessment
Complete before work starts. Redo it when the work or the conditions change.
One card per crew, per task, per day. If the task changes, the weather turns, or a new crew arrives, start a new card.
Check this yourself. This card is the field level assessment. It is not a substitute for the formal hazard assessment of the task, and an auditor will expect to see both, with this card referencing the formal one.
Job and crew
	Date
	

	Time started
	

	Site or location
	

	Task being performed today
	

	Supervisor on site
	

	Formal hazard assessment reference
	

	Weather and ground conditions
	


Conditions check
	Done
	Check

	☐
	Everyone in the crew is fit for duty and has said so.

	☐
	Everyone has the training and tickets for the task they are doing today.

	☐
	Required permits are in hand and current.

	☐
	Emergency plan, muster point and nearest medical facility are known to the crew.

	☐
	Communication has been checked, and there is a plan for the areas with no signal.

	☐
	Other crews or trades working nearby have been identified and spoken to.

	☐
	Overhead and buried services have been identified and located.

	☐
	Equipment has had its pre use inspection completed today.


Energy sources and exposures present today
	☐  Working at height
	☐  Line of fire
	☐  Pinch and crush points

	☐  Moving equipment or vehicles
	☐  Traffic and public exposure
	☐  Electrical

	☐  Stored or pressurized energy
	☐  Hot work or ignition sources
	☐  Confined space

	☐  Excavation or trenching
	☐  Unstable ground or slopes
	☐  Hazardous or controlled products

	☐  Noise
	☐  Dust or airborne contaminants
	☐  Cold or heat stress

	☐  Manual lifting and awkward postures
	☐  Wildlife
	☐  Working alone or in isolation


Task steps, hazards and controls
	Step of the job
	Hazard
	Risk L / M / H
	Control we are using
	Who

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Personal protective equipment required today
	☐  Hard hat
	☐  Safety glasses
	☐  Face shield

	☐  Hearing protection
	☐  Safety footwear
	☐  High visibility clothing

	☐  Gloves, type specified
	☐  Fall protection harness
	☐  Respirator, type specified

	☐  Flame resistant clothing
	☐  Fire extinguisher on site
	☐  Gas monitor


Changes during the shift
	Time
	What changed
	New hazard
	What we did about it

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


Stop work
Every worker on this crew has the authority to stop the work if a hazard is not controlled, and nobody will be disciplined for using it. If work is stopped, record it above and tell the supervisor immediately.
Crew sign on
By signing, I confirm I took part in this assessment, I understand the hazards and controls listed, and I know I can stop the work.
	Printed name
	Signature
	Time on

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


Supervisor review
	Supervisor

	


	Date
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